,WIDTH##LENGTH##MILLIMETERS,WD##LENGTH##MILLIMETERS,VELOCITY##HVAC_VELOCITY##METERS_PER_SECOND,URL EN##OTHER##,URL[-1010104]##OTHER##,Type Image[-1152384]##OTHER##,TOP SPIGOT DIAMETER INPUT##LENGTH##MILLIMETERS,TOP SPIGOT DEPTH##LENGTH##MILLIMETERS,TOP SPIGOT##OTHER##,SIDE SPIGOT DIAMETER INPUT##LENGTH##MILLIMETERS,SIDE SPIGOT DEPTH##LENGTH##MILLIMETERS,SIDE SPIGOT##OTHER##,PRESSURE##HVAC_PRESSURE##PASCALS,PLENUM##OTHER##,Model[-1010109]##OTHER##,Manufacturer[-1010108]##OTHER##,HEIGHT##LENGTH##MILLIMETERS,HD##LENGTH##MILLIMETERS,Description EN##OTHER##,Description[-1010103]##OTHER##,Default Elevation[-1154647]##LENGTH##MILLIMETERS,BW##LENGTH##MILLIMETERS,BH##LENGTH##MILLIMETERS,AR##OTHER##,AMB-AP-F22-D/DK##OTHER##,AIR FLOW SIDE##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,AIR FLOW##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR
AMB F 22,500.000000000000,494.000000000000,0.000000000000,https://aerogrammi.gr/en/products/wall-mounted/item/72-amb-f22,https://aerogrammi.gr/el/proionta/stomia-toixou/item/19-amb-f22,AMB F 22.jpg,150.000000000000,40.000000000000,1,150.000000000000,40.000000000000,1,0.000000000000,1,AMB F22 2 (ROWS)/AMB-AP-F22-D/DK,AEROGRAMMI,80.000000000000,74.000000000000,"Jet nozzle, made by plastic, with adjustable head in any direction. Active diameter 22mm. It is produced only in some colors. For wall (for cooling and heating) or ceiling (only for heating, for air-curtain or to avoid condensation in glass surfaces) installation.","Ακροφύσιο μεγάλου βεληνεκούς (τζετ), από πλαστικό, με ρυθμιζόμενη κεφαλή προς όλες τις κατευθύνσεις. Ενεργή διάμετρος 22mm. Παράγεται σε συγκεκριμένα χρώματα, δεν βάφεται. Τοποθετείται σε τοίχο ή στην οροφή αν χρησιμοποιηθεί για δημιουργία αεροκουρτίνας ή για την αποφυγή συγκέντρωσης συμπυκνωμάτων σε τζαμαρίες.",0.000000000000,512.000000000000,92.000000000000,6,0,0.000000000000,0.000000000000
