,WD##LENGTH##MILLIMETERS,VELOCITY##HVAC_VELOCITY##METERS_PER_SECOND,URL EN##OTHER##,URL##OTHER##,Type Image##OTHER##,TOP SPIGOT DEPTH##LENGTH##MILLIMETERS,TOP SPIGOT##OTHER##,TOP SPIGOT DIAMETER INPUT##LENGTH##MILLIMETERS,SIDE SPIGOT DIAMETER INPUT##LENGTH##MILLIMETERS,SIDE SPIGOT DEPTH##LENGTH##MILLIMETERS,SIDE SPIGOT##OTHER##,PRESSURE##HVAC_PRESSURE##PASCALS,PLENUM##OTHER##,Model##OTHER##,Manufacturer##OTHER##,HD##LENGTH##MILLIMETERS,Description EN##OTHER##,Description##OTHER##,BOX WIDTH##LENGTH##MILLIMETERS,BOX HEIGHT##LENGTH##MILLIMETERS,AR##OTHER##,WIDTH##LENGTH##MILLIMETERS,HEIGHT##LENGTH##MILLIMETERS,Default Elevation##LENGTH##MILLIMETERS,AMB-AP-F22-D/DK##OTHER##,AIR FLOW TOP##HVAC_AIR_FLOW##LITERS_PER_SECOND,AIR FLOW SIDE##HVAC_AIR_FLOW##LITERS_PER_SECOND
AMB F22 (row2),494.000000000000,0.000000000000,https://www.aerogrammi.gr/en/products/wall-mounted/item/72-amb-f22,https://www.aerogrammi.gr/el/proionta/stomia-toixou/item/19-amb-f22,AMB.jpg,40.000000000000,1,150.000000000000,150.000000000000,40.000000000000,0,0.000000000000,1,AMB F22 (row2),AEROGRAMMI A.E,154.000000000000,"Jet nozzle, made by plastic, with adjustable head in any direction. Active diameter 22mm. It is produced only in some colors. For wall (for cooling and heating) or ceiling (only for heating, for air-curtain or to avoid condensation in glass surfaces) installation.","Ακροφύσιο μεγάλου βεληνεκούς (τζετ), από πλαστικό, με ρυθμιζόμενη κεφαλή προς όλες τις κατευθύνσεις. Ενεργή διάμετρος 22mm. Παράγεται σε συγκεκριμένα χρώματα, δεν βάφεται. Τοποθετείται σε τοίχο ή στην οροφή αν χρησιμοποιηθεί για δημιουργία αεροκουρτίνας ή για την αποφυγή συγκέντρωσης συμπυκνωμάτων σε τζαμαρίες.",512.000000000000,172.000000000000,6,500.000000000000,160.000000000000,0.000000000000,0,0.000000000000,0.000000000000
